|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SEER500** | **22CH**  **Mode1** | **18CH**  **Mode2** | **DMX Value** | **Funciton** |
| Dimmer | 1 | 1 | 0---255 | Darkness----->Bright |
| Dimmer FINE | 2 |  | 0---255 |
| Strobe | 3 | 2 | 0---3  4---103  104---107  108---207  208---212  213---225  226---238  239---251  252---255 | Closed  Slow Strobe--->Fast Strobe  Open  Slow Pulsation--->Fast Pulsation  Open  Random Slow Strobe  Random Medium Strobe  Random Fast Strobe  Open |
| Color | 4 | 3 | 0---4  5---8  9---12  13---17  18---21  22---55  26---29  30--- 34  35--- 38  39---42  43---46  47---51  52---55  56---59  60---63  64---68  69---72  73---76  77---81  82---85  86---89  90---93  94---98  99---102  103---106  107---110  111—115  116---119  120---123  124--- 127  128---191  192---255 | WHITE  WHITE + RED  RED  RED + ORANGE  ORANGE  ORANGE + AQUAMARI  AQUAMARINE  AQUAMARINE + GREEN  GREEN  GREEN + LIGHT GREEN  LIGHT GREEN  LIGHT GREEN + LAVEN  LAVENDER  LAVENDER + PINK  PINK  PINK + YELLOW  YELLOW  YELLOW + MAGENTA  MAGENTA  MAGENTA + CYAN  CYAN  CYAN + CTO 260  CTO 260  CTO 260 + CTO 190  CTO 190  CTO 190 + CTB 8000  CTB 8000  CTB 8000 + BLUE  BLUE  BLUE + WHITE  **CW SlowRotation---->FastRotation**  **CCW FastRotation---->Slow Rotation** |
| Gobo1(Fixed Gobo) | 5 | 4 | 0---3  4---7  8---11  12---15  16---19  20---23  24---27  28---31  32---35  36---39  40---43  44---47  48---51  52--- 55  56---59  60---63  64---67  68---71  72---113  114---117  118---159  160---166  167---172  173---179  180---185  186--- 191  192---198  199---204  205---211  212---217  218---223  224---230  231---236  237---243  244---249  250---255 | WHITE  GOBO 1  GOBO 2  GOBO 3  GOBO 4  GOBO 5  GOBO 6  GOBO 7  GOBO 8  GOBO 9  GOBO 10  GOBO 11  GOBO 12  GOBO 13  GOBO 14  GOBO 15  GOBO 16  GOBO 17  **CW SlowRotation------>FastRotation**  **WHITE**  **CCW FastRotation------>SlowRotation**  GOBO 2 Shake Slow---->Fast  GOBO 3 Shake Slow---->Fast  GOBO 4 Shake Slow---->Fast  GOBO 5 Shake Slow---->Fast  GOBO 6 Shake Slow---->Fast  GOBO 7 Shake Slow---->Fast  GOBO 8 Shake Slow---->Fast  GOBO 9 Shake Slow---->Fast  GOBO10 Shake Slow---->Fast  GOBO11 Shake Slow---->Fast  GOBO12 Shake Slow---->Fast  GOBO13 Shake Slow---->Fast  GOBO14 Shake Slow---->Fast  GOBO15 Shake Slow---->Fast  GOBO16 Shake Slow---->Fast |
| Gobo2 Select | 6 | 5 | 0---9  10--- 20  21--- 29  30--- 39  40--- 49  50--- 59  60--- 69  70--- 79  80--- 89  90---104  105---119  120---134  135---149  150---164  165---179  180---194  195---209  210---255 | WHITE  GOBO1  GOBO2  GOBO3  GOBO4  GOBO5  GOBO6  GOBO7  GOBO8  GOBO1 Shake Slow---->Fast  GOBO2 Shake Slow---->Fast  GOBO3 Shake Slow---->Fast  GOBO4 Shake Slow---->Fast  GOBO5 Shake Slow---->Fast  GOBO6 Shake Slow---->Fast  GOBO7 Shake Slow---->Fast  GOBO8 Shake Slow---->Fast  CCW SlowRotation------> FastRotation |
| GOBO2  index Rotation | 7 | 6 | 0---127  128---191  192---255 | Position 0°---->360°(FINE in CH8)  **CW SlowRotation------> FastRotation**  **CCWFastRotation------>SlowRotation** |
| GOBO2 indexRotation FINE | 8 |  | 0---255 | GOBO2 index Rotation FINE |
| PRISM | 9 | 7 | 0---127  128--255 | EXCLUDED  INSERTED |
| PRISM Rotation | 10 | 8 | **0---127**  **128---190**  **191---194**  **195---255** | **Position 0°---->360°**  **CW FastRotation------> SlowRotation**  **STOP**  **CCW Slow Rotation------>Fast Rotation** |
| FORST | 11 | 9 | 0---255 | EXCLUDED------>INSERTED |
| FOCUS | 12 | 10 | 0---255 |  |
| FOCUS FINE | 13 |  | 0---255 |
| ZOOM | 14 | 11 | 0---255 |  |
| ZOOM FINE | 15 |  | 0---255 |
| PAN(X) | 16 | 12 | 0---255 |  |
| PAN(X) FINE | 17 | 13 | 0---255 |
| TILTE(Y) | 18 | 14 | 0---255 |  |
| TILTE(Y) FINE | 19 | 15 | 0---255 |
| P/T SPEED | 20 | 16 | 0---128  129---170  171---211  212---255 | Fastest------->Slowest  Slow Speed ( 1/3 MaxSpeed)  Medium Speed ( 1/2 MaxSpeed)  Fast Speed (Fastest Speed) |
| Lamp Control | 21 | 17 | 0---32  33---64  65---96  97---128  129---160  161---193  194---225  226---255 | Undefined  LAMP ON(>4s)  Undefined  LAMP OFF(>4s)  Undefined  HALF POWER  Undefined  FULL POWER |
| Control | 22 | 18 | 0---127  128---255 | Undefined  Reset ALL( >4s) |

\*NOTE:关闭灯泡后，请勿立即又打开灯泡，请等待大于2分钟之后再点灯泡。如果无法点亮灯泡，试试给灯泡一次“关灯泡”信号，然后再去点灯泡。