|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ARES-B4** | **20CH****Mode1** | **17CH****Mode2** | **DMX Value** | **Funciton** |
| Dimmer | 1 | 1 | 0---255 | Darkness----->Bright |
| Dimmer FINE | 2 |  | 0---255 |
| Strobe | 3 | 2 | 0---34---103104---107108---207208---212213---225226---238239---251252---255 | ClosedSlow Strobe--->Fast StrobeOpenSlow Pulsation--->Fast PulsationOpenRandom Slow StrobeRandom Medium StrobeRandom Fast StrobeOpen |
| Color | 4 | 3 | 0---910---1920--- 2930--- 3940---4950---59 60---6970---7980---8990---99100--- 109110---119120---129130---139140---149150---159160-- 207208---255 | WhiteColor1+WhiteColor1Color1 + Color2Color2Color2 + Color3Color3Color3 + Color4Color4Color4 + Color5Color5Color5 + Color6Color6Color6 + Color7Color7Color7 + WHITECW Rotation Slow--->FastCCW Rotation Fast--->Slow |
| Fixed Gobo | 5 | 4 | 0---34---78---1112---1516---1920---2324---2728---3132---3536---7677---8081---121122---138139---155156---172173---189190---206207---223224---230231---255 | WHITEGOBO 1GOBO 2GOBO 3GOBO 4GOBO 5GOBO 6GOBO 7GOBO 8CW SlowRotation------>FastRotationWHITECCW SlowRotation------> FastRotationGOBO 1 Shake Slow---->FastGOBO 2 Shake Slow---->FastGOBO 3 Shake Slow---->FastGOBO 4 Shake Slow---->FastGOBO 5 Shake Slow---->FastGOBO 6 Shake Slow---->FastGOBO 7 Shake Slow---->FastGOBO 8 Shake Slow---->Fast |
| Gobo1 Select | 6 | 5 | 0---78--- 1516---2324--- 3132--- 3940--- 4748---5960---8081---101102--- 122123--- 143 144---164 165---189190--- 222223--- 255 | WHITEGOBO 1GOBO 2GOBO 3GOBO 4GOBO 5GOBO 6GOBO 1 Shake Slow---->FastGOBO 2 Shake Slow---->FastGOBO 3 Shake Slow---->FastGOBO 4 Shake Slow---->FastGOBO 5 Shake Slow---->FastGOBO 6 Shake Slow---->FastCW SlowRotation------>FastRotationCCW SlowRotation------> FastRotation |
| GOBO1index Rotation | 7 | 6 | 0---127128---191192---255 | Position 0°---->360°(FINE in CH8)**CW SlowRotation------> FastRotation****CCWFastRotation------>SlowRotation** |
| GOBO1indexRotation FINE | 8 |  | 0---255 | GOBO1 index Rotation FINE |
| PRISM1 | 9 | 7 | 0---127128--255 | EXCLUDEDINSERTED |
| PRISM1 Rotation | 10 | 8 | **0---127****128---190****191---194****195---255** | **Position 0°---->360°****CW FastRotation------> SlowRotation****STOP****CCW Slow Rotation------>Fast Rotation** |
| FORST | 11 | 9 | 0---127128---255 | EXCLUDEDINSERTED |
| FOCUS | 12 | 10 | 0---255 |  |
| FOCUS FINE | 13 |  | 0---255 |
| PAN(X) | 14 | 11 | 0---255 |  |
| PAN(X) FINE | 15 | 12 | 0---255 |
| TILTE(Y)  | 16 | 13 | 0---255 |  |
| TILTE(Y) FINE | 17 | 14 | 0---255 |
| P/T SPEED | 18 | 15 | 0---128129---170171---211212---255 | Fastest------->SlowestSlow Speed ( 1/3 MaxSpeed)Medium Speed ( 1/2 MaxSpeed)Fast Speed (Fastest Speed) |
| Lamp Control | 19 | 16 | 0---3233---6465---9697---128129---160161---193194---225226---255 | UndefinedUndefinedUndefinedUndefinedUndefinedUndefinedUndefinedUndefined |
| Control | 20 | 17 | 0---127128---255 | UndefinedReset ALL( >4s) |

\*NOTE:关闭灯泡后，请勿立即又打开灯泡，请等待大于2分钟之后再点灯泡。如果无法点亮灯泡，试试给灯泡一次“关灯泡”信号，然后再去点灯泡。