|  |  |  |  |
| --- | --- | --- | --- |
| **OA-7000W\_II V1.1 NE** | **16CH**  **MODE1** | **DMX VALUE** | **FUNCTION** |
| Dimmer | 1 | 0--255 | [Brightness](app:ds:brightness)--->Darkness |
| Strobe | 2 | 0---7  8---65  66---71  72---127  128---133  134---189  190--195  196--250  251--255 | Undefined  Slow Strobe----->fastStrobe  Undefined  Undefined  Undefined  Undefined  Undefined  Random Strobe  Undefined |
| Shutter | 3 | 0---255 | Close---->Open |
| Cyan | 4 | 0---255 | EXCLUDED---->INSERTED |
| Magenta | 5 | 0---255 | EXCLUDED---->INSERTED |
| Yellow | 6 | 0---255 | EXCLUDED---->INSERTED |
| Color Macro | 7 | 0---255 |  |
| Forst | 8 | 0---255 | EXCLUDED---->INSERTED |
| Zoom | 9 | 0---255 |  |
| PAN(x) | 10 | 0---255 |  |
| PAN(X) FINE | 11 | 0---255 |
| TILTE(Y) | 12 | 0---255 |  |
| TILTE(Y) FINE | 13 | 0---255 |
| P/T Speed | 14 | 0---128  129---170  171---211  212---255  252---255 | Fastest------->Slowest  SlowSpeed (1/3 MaxSpeed)  MediumSpeed (1/2 MaxSpeed)  Fast Speed (Fastest Speed)  Darkness when moving |
| Lamp Control | 15 | 0---32  33---64  65---96  97---128  129---160  161---193  194---225  226---255 | Undefined  LAMP OFF( > 3s)  Undefined  LAMP ON( > 3s)  Undefined  Undefined  Undefined  Undefined |
| Control | 16 | 0---127  128---153  154---179  180---205  206---231  232---255 | Undefined  Undefined  Undefined  Undefined  Undefined  Reset ALL( > 3s) |

\*NOTE:

1.关闭灯泡后，请勿立即又打开灯泡，请等待大于5分钟之后再点灯泡。如果无法点亮灯泡，试试给灯泡一次“关灯泡”信号，然后再去点灯泡。

2.每次点亮灯泡后，需要等待20秒后，方可调光，和变功率。