|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **OA-3800ProII****V1.1 NEW** | **34CH****MODE1** | **29CH****MODE2** | **DMX VALUE** | **FUNCTION** |
| Dimmer | 1 | 1 | 0--255 | Brightness--->Darkness |
| Dimmer FINE | 2 |  | 0--255 |
| Strobe,Shutter | 3 | 2 | 0---34---103104---107108---207208---212213---225226---238239---251252---255 | CloseSlow Strobe--->Fast StrobeOpenSlowPuls---->Fast PulsOpenRandom Slow StrobeRandom Medium StrobeRandom Fast StrobeOpen |
| Color | 4 | 3 | 0---1112---2324--- 3536--- 4748--- 5960---71 72--- 8384---9596---107108---119120--- 131132---143144---155156--- 171172--- 213214--- 255 | WhiteColor1+WhiteColor1Color1 + Color2Color2Color2 + Color3Color3Color3 + Color4Color4Color4 + Color5Color5Color5 + Color6Color6Color6 + WhiteCW Rotation Slow--->FastCCW Rotation Fast--->Slow |
| Cyan | 5 | 4 | 0---255 | EXCLUDED---->INSERTED |
| Magenta | 6 | 5 | 0---255 | EXCLUDED---->INSERTED |
| Yellow | 7 | 6 | 0---255 | EXCLUDED---->INSERTED |
| Color Macro | 8 |  | 0---255 |  |
| Gobo1 Select | 9 | 7 | 0---910--- 2021--- 2930---3940--- 4950--- 5960---8586---111 112---137138---163164---189190---222223---255 | WhiteGobo1Gobo2Gobo3Gobo4Gobo5Gobo1 Shake Slow--->FastGobo2 Shake Slow--->FastGobo3 Shake Slow--->FastGobo4 Shake Slow--->FastGobo5 Shake Slow--->FastCW Rotation Slow---->FastCCW Rotation Fast--->Slow |
| Gobo1 Index Rotating | 10 | 8 | 0---127128---191192---255 | 0°----->360°(Fine in CH11)CW Rotation Slow--->FastCCW Rotation Fast--->Slow |
| Gobo1 Index Rotating FINE | 11 |  | 0---255 |  |
| Animation | 12 | 9 | 0---255 | EXCLUDED---->INSERTED |
| Animation Rotation | 13 | 10 | 0---127128---191192---255 | 0°---->360°CW Rotating Slow---FastCCW Rotation Fast---Slow |
| IRIS | 14 | 11 | 0---128129---131132---171172---211212---251252---255 | MAX----->MINCloseSlow Puls---->Fast PulsSlow Puls Fast Close---->Fast Puls Fast CloseSlow Puls Fast Open---->Fast Puls Fast OpenOpen |
| BLADE1 | 15 | 12 | 0---255 | EXCLUDED---->INSERTED |
| BLADE2 | 16 | 13 | 0---255 | EXCLUDED---->INSERTED |
| BLADE3 | 17 | 14 | 0---255 | EXCLUDED---->INSERTED |
| BLADE4 | 18 | 15 | 0---255 | EXCLUDED---->INSERTED |
| BLADE5 | 19 | 16 | 0---255 | EXCLUDED---->INSERTED |
| BLADE6 | 20 | 17 | 0---255 | EXCLUDED---->INSERTED |
| BLADE7 | 21 | 18 | 0---255 | EXCLUDED---->INSERTED |
| BLADE8 | 22 | 19 | 0---255 | EXCLUDED---->INSERTED |
| FRAMING ROTATION | 23 | 20 | 0---255 |  |
| Focus | 24 | 21 | 0---255 |  |
| Focus FINE | 25 |  | 0---255 |
| Zoom | 26 | 22 | 0---255 |  |
| Zoom FINE | 27 |  | 0---255 |
| PAN(x) | 28 | 23 | 0---255 |  |
| PAN(X) FINE | 29 | 24 | 0---255 |
| TILTE(Y) | 30 | 25 | 0---255 |  |
| TILTE(Y) FINE | 31 | 26 | 0---255 |
| P/T Speed | 32 | 27 | 0---128129---170171---211212---255252---255 | Fastest------->SlowestSlowSpeed (1/3 MaxSpeed)MediumSpeed (1/2 MaxSpeed) Fast Speed (Fastest Speed)Darkness when moving |
| Lamp Control | 33 | 28 | 0---3233---6465---9697---128129---160161---193194---225226---255 | UndefinedLAMP OFF( > 3s)UndefinedLAMP ON( > 3s)UndefinedLOW POWER( > 3s)UndefinedFULL POWER( > 3s) |
| Control | 34 | 29 | 0---127128---153154---179180---205206---231232---255 | UndefinedUndefinedUndefinedUndefinedUndefinedReset ALL( > 3s) |

\*NOTE:关闭灯泡后，请勿立即又打开灯泡，请等待大于2分钟之后再点灯泡。如果无法点亮灯泡，试试给灯泡一次“关灯泡”信号，然后再去点灯泡。